Bill of Quantities
	Item No.
	Item Description
	No.
	Qty.
	Rate In Figure
	Rate In Word
	Amount
	Remarks

	1
	Insurance of works, plants, materials, loss and damage to equipment’s, Contractor’s workmen and employees and third-party insurance against damage to other persons and property. [GCC 19.1] and other miscellaneous works
	Ps
	1.00
	[bookmark: _GoBack] 
	 
	 
	 

	2
	Provide and installation of project information board of size as per instruction of site architect/ engineer.
	Ps
	1.00
	 
	 
	 
	 

	 
	CIVIL WORKS
	 
	 
	 
	 
	 
	 

	1
	Earthwork in excavation in trenches, foundation etc. in soft soil as per specification, drawings & instruction of site engineer
	Cum
	26.15
	 
	 
	 
	 

	2
	Providing and fixing with the river gravel per drawing and technical specifications.
	Cum
	9.36
	 
	 
	 
	 

	3
	Providing and laying of Stone soling with thick stones and packing with smaller stone on prepared surface as per drawing and technical specifications.
	Cum
	10.27
	 
	 
	 
	 

	4
	Providing and laying of Plain Cement Concrete in Structure as per drawing and technical specifications. Grade M15 
	Cum
	4.23
	 
	 
	 
	 

	5
	Providing 38 mm Screeding as per drawing and instruction of Engineers.
	Sqm
	40.80
	 
	 
	 
	 

	6
	Stone masonry work in cement mortar 1:4 including 10 m lead and 5 m lift
	Cum
	21.76
	 
	 
	 
	 

	7
	Plain cement Concrete (PCC) 1:2:4 for RCC structure works with approved quality of cement, sand and crushed stone aggregate including mixing, laying, curing etc. including 30 m lead all complete in approval of site architect/ engineer.
	Cum
	10.36
	 
	 
	 
	 

	8
	TMT steel reinforcement bar of Fe 500 grade including straightening, cleaning, cutting, binding & fixing in position with annealed tying binding wire as per drawing, design & instruction all complete.
	Kg.
	664.82
	 
	 
	 
	 

	9
	Providing form work for beam and Column as per drawing, design & instruction all complete.
	Sqm
	63.95
	 
	 
	 
	 

	10
	Providing and laying of Double Layer Hollow Concrete Block Structure as per design, drawing, technical specifications and instruction of site Engineers.
	Sqm
	58.26
	 
	 
	 
	 

	11
	Providing and laying of Hollow Concrete Block Structure as per drawing, technical specifications and instruction of Engineers.
	Sqm
	53.01
	 
	 
	 
	 

	12
	Supplying and installation of Steel Post with base plate, fabricated steel roof truss, members including primer and finish coat of paint complete fabricated as per approved drawings and instruction of site architect/Engineers.
	Kg.
	849.82
	 
	 
	 
	 

	13
	Supplying and installation of fabricated angle iron with primer and finish coat of paint complete fabricated as per approved drawings and instruction of site architect/Engineers.
	Kg.
	215.52
	 
	 
	 
	 

	14
	Supplying, fixing, placing of Local sallo wood chaukos as per drawings, specification and approval of Engineers. 
	Cum
	0.36
	 
	 
	 
	 

	15
	Making and fixing of wooden shutter in 38 mm for door (Dilakhapa)
	Sqm
	6.93
	 
	 
	 
	 

	16
	Making and fixing of wooden shutter in 38 mm Window frame with 5mm glass.
	Sqm
	6.48
	 
	 
	 
	 

	17
	Providing and fixing the 3*20 mm Iron plate grill in the window
	Sqm
	6.48
	 
	 
	 
	 

	18
	Providing, laying & curing 12.5 mm cement sand (1:4) Plastering on internal/external walls to perfect plumb, lines & level including raking the mortar joints and wetting the masonry surface all complete as per design drawings, specifications and instruction of the site engineer all complete.
	Sqm
	239.40
	 
	 
	 
	 

	19
	Supplying, fixing, placing of 20 mm wooden dado/Paneling as per drawings, specification and approval of engineer.
	Sqm
	47.45
	 
	 
	 
	 

	20
	Providing and laying of Double Distemper paint in plastered surface as per drawing and technical specifications.
	Sqm
	239.40
	 
	 
	 
	 

	21
	Providing and laying of Double coat Enamel paint on wooden and metal Surface as per drawing and technical specifications.
	Sqm
	42.04
	 
	 
	 
	 

	22
	Supplying and laying of Non-skid Ceramic Floor Tile as per instruction of site architect/ engineer.
	Sqm
	3.30
	 
	 
	 
	 

	23
	Supply and laying of Porcelain Wall Tile as per instruction of site architect/ engineer
	Sqm
	9.51
	 
	 
	 
	 

	24
	Providing and Fixing 16mm Granite tile in 1:4 Ratio
	Sqm
	2.10
	 
	 
	 
	 

	25
	Supplying and installation of fabricated 0.46 mm Color CGI sheet as per design, drawing, technical specifications and instruction of Engineers.
	Sqm
	72.90
	 
	 
	 
	 

	26
	Supplying and installation of fabricated 0.41mm color PGI sheet (Ridge cover) as per design, drawing, technical speciation’s and instruction of Engineers.
	Rm
	9.00
	 
	 
	 
	 

	 
	SANITORY WORK
	 
	 
	 
	 
	 
	 

	27
	Kitchen Sink Stainless Steel 37"*18" with sink cock all complete set.
	Set
	1.00
	 
	 
	 
	 

	28
	22 Inch Porcelain clay white glazed Orissa pan with low level glazed cistern complete 
	Set
	1.00
	 
	 
	 
	 

	29
	Installing the existing 2,000-litre PVC/HDPE water tank on the water tank stand, complete in all respects 
	Set
	1.00
	 
	 
	 
	 

	30
	22*16inch Porcelain clay white glaze Wash basin with pedestal and mixture complete set. 
	Set
	1.00
	 
	 
	 
	 

	31
	15mm CP Bib Cock  
	Set
	2.00
	 
	 
	 
	 

	32
	15mm C.P.Sink Cock
	Set
	1.00
	 
	 
	 
	 

	33
	 15mm C.P. Angle valve  
	Set
	3.00
	 
	 
	 
	 

	34
	 C.P. Gate valve  
	Set
	2.00
	 
	 
	 
	 

	35
	PVC Floor Trap 11x7.5cm (4" X 2½")
	Set
	1.00
	 
	 
	 
	 

	36
	PVC Grating 100mm (4")  dia  
	Set
	1.00
	 
	 
	 
	 

	37
	75 mm dia PVC Pipe 6 kg/cm2.
	Rm
	10.00
	 
	 
	 
	 

	38
	110 mm dia PVC Pipe 6 kg/cm2.
	Rm
	5.00
	 
	 
	 
	 

	39
	15 mm CPVC (Chlorinated Polyvinyl Chloride) Pipe SDR 11 CTS
	Rm
	15.00
	 
	 
	 
	 

	40
	25 mm CPVC (Chlorinated Polyvinyl Chloride) Pipe SDR 11 CTS.
	Rm
	10.00
	 
	 
	 
	 

	 
	ELECTRICAL WORKS
	 
	 
	 
	 
	 
	 

	41
	Supplying and fixing of 32 Amp 415 Volt DP Main Switch Complete Set including all complete accessories 
	Set
	1.00
	 
	 
	 
	 

	42
	Supplying and fixing of 8-way DPN DB Double Cover Complete Set including all complete accessories 
	Set
	1.00
	 
	 
	 
	 

	43
	Supplying and fixing of 6–32-amp MCB DP (double pole) Complete Set including all complete accessories 
	Set
	4.00
	 
	 
	 
	 

	44
	Supply and installation of Junction box 4"×6” including all complete accessories 
	Set
	4.00
	 
	 
	 
	 

	45
	Supply and installation 3*20 PVC insulated Copper wire including all complete accessories 
	Rm
	120.00
	 
	 
	 
	 

	46
	Supply and installation 7/22 PVC insulated Copper wire including all complete accessories 
	Rm
	100.00
	 
	 
	 
	 

	47
	Supply and installation of four gang one way switch including all complete accessories
	Set
	6.00
	 
	 
	 
	 

	48
	Supply and installation of 6/16 Amp, 2/3 Pin Power sockets with switch & indicator including all complete accessories
	Set
	10.00
	 
	 
	 
	 

	49
	 Supply and fixing of 12 watt Volt CFL Light Complete Set including all complete accessories 
	Set
	12.00
	 
	 
	 
	 

	 
	 
	Base Cost
	 
	 
	 

	 
	 
	VAT (13%)
	 
	 
	 

	 
	 
	Total w/t VAT & PS
	 
	 
	 

	 
	 
	Grand Total
	 
	 
	 



